The Gen 2 easy-Drive configuration tool is designed to provide a simple tool for configuring Gen 2 and Gen 1 easy-Drive electric actuators.

Connection type: USB-RS-485 converter with Modbus protocol (device and drivers not included)
Computer Requirements: Windows 8.1, 10, or 11

Installation of the configuration tool -
1. Ensure you have administrative rights for your computer
2. Remove the license dongle if already in a USB port.
3. Run the file "Gen2easyDriveConfigurator_V2.4.0.2.bat".
4. Follow the on-screen prompts for a full installation.
5. The command window will open and two separate installations will occur.  The first is the configuration tool itself.  The second is the driver for the license dongle.

